{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKCB-CV3"]
[]
[]
[]
[]
["","","","","EKCB07CAV3"]
["Méretek","Egység","Szélesség","mm","340"]
["","","Mélység","mm","97.0"]
["","","Magasság","mm","360"]
["Burkolat","Anyag","","","Előbevonattal ellátott fémlemez"]
["","Szín","","","Fehér"]
["Tömeg","Egység","","kg","4.00"]
["Vezetékcsatlakozások","a választható *KHW* modell áramellátásának csatlakozója + Q2L","Megjegyzés","","Kábelrész 2,5 mm2"]
["","","Mennyiség","","4+GND"]
["","A felhasználói interfésszel való csatlakoztatásra","Megjegyzés","","100 mA, 0,75 mm² - 1,25 mm² (max hossz 500m)"]
["","","Mennyiség","","2"]
["Power supply","Phase","","","1~"]
["","Frekvencia","","Hz","50"]
["","Feszültség","","V","230"]
["Áram","Javasolt biztosítékok","","A","10"]
["Notes","","","","(1) - A készülék megfelel az EN/IEC 61000-3-12 szabványnak: A fázisonként >16 A és ≤ 75 A közötti bemeneti áramú kisfeszültségű rendszerhez csatlakozó készülékek által létrehozott harmonikus áram határértékeit meghatározó európai/nemzetközi műszaki szabvány"]
["","","","","(2) - *KCB*C* és *K2CB*C* között"]
["","","","","(3) - Válassza ki az átmérőt és típust a helyi és országos előírásoknak megfelelően"]