{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P","EKSV21P1","EKSV26P","EKSV26P1"]
["Abszorber","","","","Hárfa alakú rézcső illeszték lézerhegesztésű nagy szelektivitású bevonattal ellátott alumíniumlemezzel","Hárfa alakú rézcső illeszték lézerhegesztésű nagy szelektivitású bevonattal ellátott alumíniumlemezzel","Hárfa alakú rézcső illeszték lézerhegesztésű nagy szelektivitású bevonattal ellátott alumíniumlemezzel","Hárfa alakú rézcső illeszték lézerhegesztésű nagy szelektivitású bevonattal ellátott alumíniumlemezzel"]
["Nyugalmi hőmérséklet","Max.","","°C","192","192","192","192"]
["Méretek","Egység","Szélesség","mm","85","1,006","85","1,300"]
["","","Mélység","mm","2,000","85","2,000","85"]
["","","Magasság","mm","1,006","2,000","1,300","2,000"]
["Üzemi nyomás","Max.","","bar","6","6","6","6"]
["Tömeg","Egység","","kg","33","35","42","42"]
["Felület","Szívónyílás","","m²","1.800","1.800","2.360","2.360"]
["","Abszorber","","m²","1.79","1.80","2.35","2.36"]
["","Külső","","m²","2.01","2.01","2.60","2.60"]
["Beszerelés_","","","","Függőleges","Függőleges","Függőleges","Függőleges"]
["Üvegezés","","","","Egytáblás biztonsági üveg, átlátszósága +/- 92%","Egytáblás biztonsági üveg, átlátszósága +/- 92%","Egytáblás biztonsági üveg, átlátszósága +/- 92%","Egytáblás biztonsági üveg, átlátszósága +/- 92%"]
["A tető megengedett dőlésszöge","Max.","","°","80","80","80","80"]
["","Min.","","°","15","15","15","15"]
["Burkolat","","","","Micro-therm (abszorpció: max. 96%, emisszió: kb. 5% +/-2%)","Micro-therm (abszorpció: max. 96%, emisszió: kb. 5% +/-2%)","Micro-therm (abszorpció: max. 96%, emisszió: kb. 5% +/-2%)","Micro-therm (abszorpció: max. 96%, emisszió: kb. 5% +/-2%)"]
["Mennyiség","l","","","1.3","1.3","1.7","1.7"]
["Hőleadási teljesítmény","Zéró veszteséges kollektro katékonyság η0","","%","0.781","0.710","0.784","0.710"]
["","a1 hőveszteségi együttható","","W/m².K","4.240","4.300","4.250","4.300"]
["","A hőmérséklet és az a2 hőveszteségi együttható összefüggése","","W/m².K²","0.006","0.006","0.007","0.006"]
["","Hőkapacitás","","kJ/K","4.9","4.9","6.5","6.5"]