{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK12-14AW1"]
[]
[]
[]
[]
["","","","","","EPSK12ARW1","EPSK14ARW1"]
["Méretek","Egység","","Magasság","mm","1123","1123"]
["","","","Szélesség","mm","1330","1330"]
["","","","Mélység","mm","604","604"]
["Tömeg","Egység","","","kg","191","191"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","96.3","96.3"]
["","","Hűtés","Magas","m³/perc","96.3","96.3"]
["Működési tartomány","Hűtés","","Min.","°C száraz hőm.","10","10"]
["","","","Max.","°C száraz hőm.","43","43"]
["Üzemi tartomány","Használati meleg víz","","Min.","°C száraz hőm.","-28","-28"]
["Működési tartomány","Használati meleg víz","","Max.","°C száraz hőm.","40","40"]
["Hangteljesítmény szintje","Fűtés","","Névl.","dB(A)","52 (1)","52 (1)"]
["","Hűtés","","Névl.","dB(A)","62 (2)","63 (2)"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","38 (1)","38 (1)"]
["","Hűtés","","Névl.","dB(A)","47 (2)","48 (2)"]
["Hűtőközeg","Típus","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["","Töltet","","","tCO2Eq","0.0038","0.0038"]
["","Töltet","","","kg","1.25","1.25"]
["Csőcsatlakozások","Szintkülönbség","IU - OU","Max.","m","10","10"]
["Áramellátás","Megnevezés","","","","W1","W1"]
["","fázis","","","","3~","3~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","400","400"]
["Áram","Javasolt biztosítékok","","","A","16","16"]
["Notes","","","","","(1) - LWC 47-55°C értéken mérve; Tkörny DB/WB 7°C/ 6°C.","(1) - LWC 47-55°C értéken mérve; Tkörny DB/WB 7°C/ 6°C."]
["","","","","","(2) - LWC 12-7°C értéken mérve; Tkörny 35°C.","(2) - LWC 12-7°C értéken mérve; Tkörny 35°C."]
["","","","","","(3) - 1 1/4” terepi csővezetékekhez","(3) - 1 1/4” terepi csővezetékekhez"]
["","","","","","(4) - 1 1/2” terepi csővezetékekhez","(4) - 1 1/2” terepi csővezetékekhez"]