{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB10A / EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPSXB10P30AF / EPSK06ARV3","EPSXB10P50AF / EPSK06ARV3","EPSXB10P30AF / EPSK08ARV3","EPSXB10P50AF / EPSK08ARV3","EPSXB10P30AF / EPSK10ARV3","EPSXB10P50AF / EPSK10ARV3"]
["Beltéri egység","","","","","EPSXB10P30AF","EPSXB10P50AF","EPSXB10P30AF","EPSXB10P50AF","EPSXB10P30AF","EPSXB10P50AF"]
["Fűtőkapacitás","Névl.","","","kW","5.81 (1)","5.81 (1)","7.62 (1)","7.62 (1)","8.11 (1)","8.11 (1)"]
["Hűtési teljesítmény","Névl.","","","kW","6.00 (2), 6.37 (3)","6.00 (2), 6.37 (3)","6.89 (2), 6.37 (3)","6.89 (2), 6.37 (3)","7.84 (2), 6.37 (3)","7.84 (2), 6.37 (3)"]
["Elektromos bemenet","Fűtés","","Névl.","kW","1.12 (1)","1.12 (1)","1.52 (1)","1.52 (1)","1.64 (1)","1.64 (1)"]
["","Hűtés","","Névl.","kW","1.55 (2), 1.13 (3)","1.55 (2), 1.13 (3)","1.85 (2), 1.13 (3)","1.85 (2), 1.13 (3)","2.17 (2), 1.13 (3)","2.17 (2), 1.13 (3)"]
["Áramfelvétel","Háztartási melegvíz 10°C és 50°C között","","Névl.","kWh","3.42","5.25","3.42","5.25","3.42","5.25"]
["Felmelegedési idő 10°C-ról 50°C-ra","ó","","","","2 h 21 min","3 h 34 min","2 h 21 min","3 h 34 min","2 h 21 min","3 h 34 min"]
["COP","","","","","5.19 (1)","5.19 (1)","5.01 (1)","5.01 (1)","4.94 (1)","4.94 (1)"]
["EER","","","","","3.87 (2), 5.63 (3)","3.87 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.62 (2), 5.63 (3)","3.62 (2), 5.63 (3)"]
["Használati meleg víz előállítás","Általános","","Terhelési profil","","L","XL","L","XL","L","XL"]
["","Átlagos klíma","","Vízmelegítés energiahatékonysági osztály","","A","A+","A","A+","A","A+"]
["Felületfűtés","55°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","3.91","3.91","3.97","3.97","4.02","4.02"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++","A+++","A+++","A+++"]
["","35°C kilépő víz hőmérséklet, átlagos klíma","Általános","SCOP","","5.12","5.12","5.15","5.15","5.15","5.15"]
["","","","Szezonális felületfűtési hatékonysági osztály","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Feltétel: Tkörny DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(2) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(2) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(2) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(2) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm.","(2) - Hűtés: EW 12℃; LW 7℃; környezeti körülmények: 35°C száraz hőm."]
["","","","","","(3) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm.","(3) - Hűtés: EW 23℃; LW 18℃; környezeti körülmények: 35°C száraz hőm."]