{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB10A"]
[]
[]
[]
[]
["","","","","","EPSXB10P30AF","EPSXB10P50AF"]
["Burkolat","Szín","","","","Közlekedési fehér (RAL9016), Grafitfekete (RAL9011), Mélyfekete (RAL9005)","Közlekedési fehér (RAL9016), Grafitfekete (RAL9011), Mélyfekete (RAL9005)"]
["","Anyag","","","","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén"]
["Méretek","Egység","","Magasság","mm","1914","1906"]
["","","","Szélesség","mm","590","785"]
["","","","Mélység","mm","671","837"]
["Tömeg","Egység","","","kg","87.0","109"]
["PED","Kategória","","","","4.3 cikk","4.3 cikk"]
["Hangteljesítmény szintje","Névl.","","","dB(A)","49.0","49.0"]
["Hangnyomás szint","Névl.","","","dB(A)","35.0","35.0"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["","Hűtés","Környezeti","Min.","°C száraz hőm.","0 (3)","0 (3)"]
["","","Vízoldal","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","230","230"]
["Elektromos fűtő","Áramellátás","","Név","","6V / 9W","6V / 9W"]
["","","","Fázis","","1~ / 3~","1~ / 3~"]
["","","","Frekvencia","Hz","50","50"]
["","","","Feszültség","V","230/400","230/400"]
["Elektromos fűtőtest","Javasolt biztosítékok","","","A","0 (4)","0 (4)"]
["Notes","","","","","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség"]
["","","","","","(2) - Minimális szükséges mennyiség, az egységben található mennyiségen kívül","(2) - Minimális szükséges mennyiség, az egységben található mennyiségen kívül"]
["","","","","","(3) - Az üzemi határértekekért hivatkozzon a rajzra","(3) - Az üzemi határértekekért hivatkozzon a rajzra"]
["","","","","","(4) - Hivatkozzon a vezetékezési diagramra és a telepítési útmutatóra a helyes, ajánlott biztosítékért az áramellátás és a hálózat csatlakoztatásához","(4) - Hivatkozzon a vezetékezési diagramra és a telepítési útmutatóra a helyes, ajánlott biztosítékért az áramellátás és a hálózat csatlakoztatásához"]