{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Méretek","Egység","","Magasság","mm","740"]
["","","","Szélesség","mm","884"]
["","","","Mélység","mm","388"]
["Tömeg","Egység","","","kg","58.5"]
["Működési tartomány","Hűtés","","Min.","°C száraz hőm.","10"]
["","","","Max.","°C száraz hőm.","43"]
["Üzemi tartomány","Használati meleg víz","","Min.","°C száraz hőm.","-25"]
["Működési tartomány","Használati meleg víz","","Max.","°C száraz hőm.","35"]
["Hangteljesítmény szintje","Fűtés","","Névl.","dB(A)","58 (1)"]
["","Hűtés","","Névl.","dB(A)","61 (1)"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","44 (1)"]
["","Hűtés","","Névl.","dB(A)","48 (1)"]
["Hűtőközeg","Típus","","","","R-32"]
["","GWP","","","","675.0"]
["","Töltet","","","tCO2Eq","1.01"]
["","Töltet","","","kg","1.50"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6"]
["","Gáz","","Külső átm.","mm","15.9"]
["","Ürítés","","külső átm.","mm","18"]
["","Szintkülönbség","IU - OU","Max.","m","20.0"]
["","Fűtés szigetelés","","","","Mind a folyadék-, mind a gázcsövek"]
["Áramellátás","Megnevezés","","","","V3"]
["","fázis","","","","1N~"]
["","Frekvencia","","","Hz","50"]
["","Feszültség","","","V","230"]
["Áram","Javasolt biztosítékok","","","A","20"]
["Notes","","","","","(1) - Hűtés Ta 35°C – LWE 18℃ ( DT = 5℃ ); Fűtés Ta DB/WB 7°C / 6°C – LWC 35℃ ( DT = 5°C )"]