{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DV37"]
[]
[]
[]
[]
["","","","","","ERLA16D2V37","ERLA16DAV37"]
["Méretek","Egység","","Magasság","mm","870","870"]
["","","","Szélesség","mm","1100","1100"]
["","","","Mélység","mm","460","460"]
["Tömeg","Egység","","","kg","101","101"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","85.0","85.0"]
["","","Hűtés","Magas","m³/perc","85","85"]
["Működési tartomány","Hűtés","","Min.","°C száraz hőm.","10","10"]
["","","","Max.","°C száraz hőm.","43","43"]
["Üzemi tartomány","Használati meleg víz","","Min.","°C száraz hőm.","-25","-25"]
["Működési tartomány","Használati meleg víz","","Max.","°C száraz hőm.","25 (1), 35 (1)","25 (1), 35 (1)"]
["Hangteljesítmény szintje","Fűtés","","Névl.","dB(A)","62.0 (2)","62.0 (2)"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","48.0 (2)","48.0 (2)"]
["Hűtőközeg","Típus","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Töltet","","","tCO2Eq","2.57","2.57"]
["","Töltet","","","kg","3.8","3.8"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.5","9.5"]
["","Gáz","","Külső átm.","mm","15.9","15.9"]
["","Ürítés","","külső átm.","mm","26","26"]
["","Szintkülönbség","IU - OU","Max.","m","30.0","30.0"]
["","Fűtés szigetelés","","","","Mind a folyadék-, mind a gázcsövek","Mind a folyadék-, mind a gázcsövek"]
["Áramellátás","Megnevezés","","","","V3","V3"]
["","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","230","230"]
["Áram","Javasolt biztosítékok","","","A","32","32"]
["Notes","","","","","(1) - További részleteket lásd az üzemi tartomány ábrán","(1) - További részleteket lásd az üzemi tartomány ábrán"]
["","","","","","(2) - A mérést a fűtőrendszerben 10 kPa nyomásesésnél, 47-55°C kimenő víz üzemi állapotban, és 20°C környezeti hőmérsékletű helyiségben végezték. DB/WB 7°C/6°.","(2) - A mérést a fűtőrendszerben 10 kPa nyomásesésnél, 47-55°C kimenő víz üzemi állapotban, és 20°C környezeti hőmérsékletű helyiségben végezték. DB/WB 7°C/6°."]