{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB12E"]
[]
[]
[]
[]
["","","","","","ETSXB12P30EG","ETSXB12P50EG","ETSXB12P30EF (Archived)","ETSXB12P50EF (Archived)"]
["Burkolat","Szín","","","","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)","Közlekedési fehér (RAL9016) / közlekedési fekete (RAL9017)"]
["","Anyag","","","","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén","Behatásoknak ellenálló polipropilén"]
["Méretek","Egység","","Magasság","mm","1891","1910","1892","1910"]
["","","","Szélesség","mm","594","792","594","792"]
["","","","Mélység","mm","644","817","644","816"]
["Tömeg","Egység","","","kg","76","100","76","100"]
["Hangteljesítmény szintje","Névl.","","","dB(A)","47.3","47.3","47.3","47.3"]
["Hangnyomás szint","Névl.","","","dB(A)","38.6","38.6","38.6","38.6"]
["Üzemi tartomány","Fűtés","Vízoldal","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Hűtés","Környezeti","Min.","°C száraz hőm.","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Vízoldal","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","230","230","230","230"]
["Notes","","","","","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség","(1) - Az EN12897 szerinti hőveszteség"]
["","","","","","(2) - Lásd az üzemi határok rajzait","(2) - Lásd az üzemi határok rajzait","(2) - Lásd az üzemi határok rajzait","(2) - Lásd az üzemi határok rajzait"]