{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Burkolat","Szín","","","","Fehér","Fehér"]
["","Anyag","","","","Műgyanta","Műgyanta"]
["Méretek","Egység","","Magasság","mm","290","340"]
["","","","Szélesség","mm","1050","1200"]
["","","","Mélység","mm","269","262"]
["Tömeg","Egység","","","kg","14","18"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","16.2","23"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","13.4","21.1"]
["","","","Alacsony","m³/perc","12.1","18.7"]
["","","Fűtés","Magas","m³/perc","16.9","23"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","14.2","20.9"]
["","","Fűtés","Alacsony","m³/perc","12.7","18.7"]
["Hangteljesítményszint","Hűtés","","","dB(A)","61","65"]
["","Fűtés","","","dB(A)","61","65"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","45","49"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","42","45"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","40","41"]
["","Fűtés","","Magas","dB(A)","45","49"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","42","45"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","40","41"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52","9.52"]
["","Gáz","","Külső átm.","mm","15.9","15.9"]
["","Ürítés","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Áramellátás","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Feszültség","","","V","220-240","220-240"]
["Standard Accessories","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Notes","","","","","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Standard Accessories","Screw cover","","","","","3"]