{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG71L8Y1B","FAQ71CVEB9 / RZQG71L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L8Y1B"]
["Felülethűtés","SEER","","","6.51","6.43","5.10","5.10"]
["","Éves energiafogyasztás","","kWh/a","366","371","652","824"]
["","Kapacitás","Pdesign","kW","6.80","6.80","9.50","12.00"]
["","Energiatakarékossági osztály","","","A++","A++","B","B"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","6.33","6.33","11.30","12.71"]
["","SCOP/A","","","4.02","4.02","3.80","3.80"]
["","Energiatakarékossági osztály","","","A+","A+","A","A"]
["","Éves energiafogyasztás","","kWh/a","2,205","2,205","4,164","4,683"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["Hűtési teljesítmény","Névl.","","kW","","6.8"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","1,000"]
["","EER","","","","3.40"]
["","COP","","","","3.70"]
["","Energiacímkézés irányelve","Hűtés","","","A"]
["","","Fűtés","","","A"]
["Fűtőkapacitás","Névl.","","kW","","7.5"]
["Notes","","","","","(1) - Az éves energiafogyasztás megfelel az 2002/31/EC energiafogyasztási direktívának"]
["","","","","","(2) - A SEER és SCOP értékek megfelelnek az EN 14825 szabvány előírásainak"]