{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXS-L"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXS50L2V1B","FBA60A2VEB9 / RXS60L2V1B"]
["Hűtési teljesítmény","Névl.","","kW","","5.70"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","826"]
["","EER","","","","3.45"]
["","COP","","","","37.10"]
["","Energiacímkézés irányelve","Hűtés","","","A"]
["","","Fűtés","","","A"]
["Fűtőkapacitás","Névl.","","kW","","7.00"]
["Notes","","","","","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(4) - Az elektromos adatokat lásd külön rajzokon"]
["Outdoor unit","","","","RXS50L2V1B"]
["Hűtési teljesítmény","Névl.","","kW","5.00"]
["Fűtőkapacitás","Névl.","","kW","5.50"]
["Névleges hatékonyság","EER","","","3.52"]
["","COP","","","38.30"]
["","Éves energiafogyasztás","","kWh","710"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A"]
["","","Fűtés","","A"]
["Felülethűtés","Energiatakarékossági osztály","","","A++"]
["","Kapacitás","Pdesign","kW","5.00"]
["","SEER","","","6.21"]
["","Éves energiafogyasztás","","kWh/a","282"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A+"]
["","Kapacitás","Pdesign","kW","4.40"]
["","SCOP/A","","","4.06"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","3.73"]
["","Éves energiafogyasztás","","kWh/a","1517"]
["Energiatakarékossági besorolás","","","","A+++ ~ D"]