{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZQ-C"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZQ200C7Y1B","FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / RZQ250C7Y1B"]
["Hűtési teljesítmény","Névl.","","kW","20.0 (1)","24.1 (1)"]
["Felülethűtés","SEER","","","5.67","5.74"]
["","Éves energiafogyasztás","","kWh/a","2,115","2,518"]
["","Kapacitás","Pdesign","kW","20.0","24.1"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","11.2","12.1"]
["","SCOP/A","","","3.68","3.76"]
["","Éves energiafogyasztás","","kWh/a","4,257","4,484"]
["Fűtőkapacitás","Névl.","","kW","23.0 (2)","26.4 (2)"]
["Notes","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m"]
["","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m"]
["","","","","(3) - Ez az érték nem tartalmazza a csökkenő kapacitást a leolvasztási művelettel.","(3) - Ez az érték nem tartalmazza a csökkenő kapacitást a leolvasztási művelettel."]