{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":12,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9)"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB9","FBA50A2VEB9","FBA60A2VEB9","FBA71A2VEB9","FBA100A2VEB","FBA125A2VEB","FBA140A2VEB"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","","","","","","14.00","15.40"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","","","","","","13.5","15.5"]
["Burkolat","Szín","","","","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)","Festés nélküli (galvanizált)"]
["","Anyag","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["Méretek","Egység","","Magasság","mm","245","245","245","245","245","245","245"]
["","","","Szélesség","mm","700","700","1000","1000","1400","1400","1400"]
["","","","Mélység","mm","800","800","800","800","800","800","800"]
["Tömeg","Egység","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","","Alacsony","m³/perc","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","","Fűtés","Magas","m³/perc","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","Fűtés","Alacsony","m³/perc","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","Külső statikus nyomás","","Névl.","Pa","30","30","30","30","40","50","50"]
["Hangteljesítményszint","Hűtés","","","dB(A)","60.0","60.0","56.0","56.0","58.0","62.0","62.0"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","35.0","35.0","30.0","30.0","34.0","37.0","37.0"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32.0","32.0","28.0","28.0","32.0","35.0","35.0"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["","Fűtés","","Magas","dB(A)","37.0","37.0","31.0","31.0","36.0","38.0","38.0"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34.0","34.0","28.0","28.0","33.0","35.0","35.0"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","mm","9.52","12.70","12.70","15.90","15.90","15.90","15.90"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Leeresztési emelési magasság","mm","","","","625","625","625","625","625","625","625"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Vezetékes távszabályzó","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","1","1","1","","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8","8"]
["","Operation manual","","","","1","1","1","","1","1","1"]
["","Clamps","","","","4","4","4","","4","4","4"]
["","Drain hose","","","","1","1","1","","1","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1","1"]
["","Screws","","","","40","40","40","","40","40","40"]
["","Sealing pads","","","","5","5","5","","5","5","5"]
["Áramellátás","fázis","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Feszültség","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Standard Accessories","Telepítési utasítás","","","","","","","1"]
["","Alátét a függesztőkerethez","","","","","","","8"]
["","Használati utasítás","","","","","","","1"]
["","Bilincsek","","","","","","","4"]
["","Leeresztő tömlő","","","","","","","1"]
["","Szigetelés a szereléshez","","","","","","","2"]
["","Az leeresztő tömlő fémbilincse","","","","","","","1"]
["","Csavarok","","","","","","","40"]
["","Tömítések","","","","","","","5"]
["Notes","","","","","","","","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]
["","","","","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","","(2) - Az elektromos adatokat lásd külön rajzokon"]