{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / FBQ35C8VEB / RZQG71L8Y1B","FBQ71C8VEB / RZQG71L8Y1B","FBQ100C8VEB / RZQG100L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L8Y1B","FBQ50C8VEB / FBQ50C8VEB / RZQG100L8Y1B","FBQ125C8VEB / RZQG125L8Y1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L8Y1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L8Y1B","FBQ140C8VEB / RZQG140L7Y1B"]
["Hűtési teljesítmény","Névl.","","kW","","6.8","9.5","","","12.0","","","13.4"]
["Felülethűtés","SEER","","","5.1","6.11","5.8","5.1","5.1","5.81","5.1","5.1"]
["","Éves energiafogyasztás","","kWh/a","467","390","574","652","652","723","824","824"]
["","Kapacitás","Pdesign","kW","6.8","6.8","9.5","9.5","9.5","12","12","12"]
["","Energiatakarékossági osztály","","","B","A++","A+","B","B","A+","B","B"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","6","6","11.3","11.3","11.3","12.71","12.71","12.71"]
["","SCOP/A","","","3.8","4.01","4.61","3.8","3.8","4.21","3.8","3.8"]
["","Energiatakarékossági osztály","","","A","A+","A++","A","A","A+","A","A"]
["","Éves energiafogyasztás","","kWh/a","2,211","2,095","3,432","4,164","4,164","4,227","4,683","4,683"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","970","1,220","","","1,575","","","2,010"]
["","EER","","","","3.50","3.89","","","3.81","","","3.33"]
["","COP","","","","3.65","4.21","","","3.83","","","3.61"]
["","Energiacímkézés irányelve","Hűtés","","","A","A","","","A"]
["","","Fűtés","","","A","A","","","A"]
["Fűtőkapacitás","Névl.","","kW","","7.5","10.8","","","13.5","","","15.5"]
["Notes","","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]
["","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]