{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / ARXM-N9"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / ARXM71N2V1B9"]
["Hűtési teljesítmény","Max.","","kW","7.05"]
["","Névl.","","kW","6.80"]
["Normál hatékonyság","Annual energy consumption","","kWh","1,083"]
["","EER","","","3.14"]
["","COP","","","3.38"]
["","Energiacímkézés irányelve","Hűtés","","B"]
["","","Fűtés","","C"]
["Fűtőkapacitás","Névl.","","kW","7.50"]
["","Max.","","kW","7.58"]
["Notes","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]