{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50AVEB / RXS50L2V1B","FCAG60AVEB / RXS60L2V1B"]
["Hűtési teljesítmény","Névl.","","kW","5.00","5.70"]
["Felülethűtés","SEER","","","6.48","6.22"]
["","Éves energiafogyasztás","","kWh/a","270","321"]
["","Kapacitás","Pdesign","kW","5.00","5.70"]
["","Energiatakarékossági osztály","","","A++","A++"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","4.36","4.71"]
["","SCOP/A","","","4.29","4.00"]
["","Energiatakarékossági osztály","","","A++","A+"]
["","Éves energiafogyasztás","","kWh/a","1,426","1,646"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","6.35","6.35"]
["","Gáz","Külső átm.","pp","12.70","12.70"]
["","Ürítés","OD","pp","VP25 (Külső átm.32, belső átm. 25)","VP25 (Külső átm.32, belső átm. 25)"]
["Normál hatékonyság","EER","","","3.55","3.48"]
["","Éves energiafogyasztás","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","Energiacímkézés irányelve","Hűtés","","A","A"]
["","","Fűtés","","A","B"]
["Fűtőkapacitás","Névl.","","kW","6.00","7.00"]
["Notes","","","","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","(4) - Az elektromos adatokat lásd külön rajzokon","(4) - Az elektromos adatokat lásd külön rajzokon"]