{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG140L7Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B"]
["Energiatakarékossági besorolás","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D"]
["Felülethűtés","SEER","","","","","","","","","","","","","5.10","5.10","6.72","","","6.44","9.70"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","","","467","467","355","","","1,249","829"]
["","Kapacitás","Pdesign","kW","","","","","","","","","","","6.80","6.80","6.80","","","13.4","13.4"]
["","Energiatakarékossági osztály","","","","","","","","","","","","","A","A","A++"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","","","","","","","","","","","6.00","6.00","6.33","","","11.6","12.0"]
["","SCOP/A","","","","","","","","","","","","","3.80","3.80","4.20","","","4.27","3.96"]
["","Energiatakarékossági osztály","","","","","","","","","","","","","A","A","A+"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","","","2,211","2,211","2,110","","","3,795","4,235"]
["Notes","","","","","","","","","","","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m"]
["","","","","","","","","","","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m"]
["","","","","","","","","","","","","","","(3) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","(3) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","","(3) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(3) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["Hűtési teljesítmény","Névl.","","kW","","","","","","","","","","","","","6.80 (1)","","","13.4 (1)","13.4 (1)"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","","","","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","","","","","3.39 (3)","","","2.50 (3)","4.29 (3)"]
["","COP","","","","","","","","","","","","","","","3.97 (3)","","","3.61 (3)"]
["","Energiacímkézés irányelve","Hűtés","","","","","","","","","","","","","","A"]
["","","Fűtés","","","","","","","","","","","","","","A"]
["Fűtőkapacitás","Névl.","","kW","","","","","","","","","","","","","7.50 (2)","","","15.5 (2)","15.5 (2)"]
["Outdoor unit","","","","","","","","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Felülethűtés","Energiatakarékossági osztály","","","","","","","","","","","","","","","","A","A"]
["","Kapacitás","Pdesign","kW","","","","","","","","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","","","","","","652","824"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","","","","","","","","","","","","","A","A"]
["","Kapacitás","Pdesign","kW","","","","","","","","","","","","","","11.3","12.7"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","","","","","","4164","4683"]
["Felülethűtés","ηs,c","","%","","","","","","","","","","","","","","","","254.6","385.1"]
["Felületfűtés (Mérsékelt éghajlat)","ηs,h","","%","","","","","","","","","","","","","","","","167.6","155.2"]