{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","FCAHG100FVEB","FCAHG125FVEB","FCAHG140FVEB","FCAHG71FVEB"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","44","45","45"]
["","","Közepes","dB(A)","39","40","41"]
["","","Alacsony","dB(A)","33","35","37"]
["","Hűtés","Medium","dB(A)","39","40","41"]
["","","Alacsony","dB(A)","33","35","37"]
["","","Magas","dB(A)","44","45","45"]
["Standard Accessories","Telepítési és használati utasítás","","","Telepítési és használati utasítás","Telepítési és használati utasítás","Telepítési és használati utasítás","Telepítési és használati utasítás"]
["","Telepítési utasítás","","","Telepítési utasítás","Telepítési utasítás","Telepítési utasítás","Telepítési utasítás"]
["Refrigerant","GWP","","","675","675","675","675"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","9.52","9.52","9.52","9.52"]
["","Gáz","Külső átm.","pp","15.9","15.9","15.9"]
["","Ürítés","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dekorációs panel 4","Méretek","Mélység","pp","950","950","950","950"]
["","","Szélesség","pp","950","950","950","950"]
["","","Magasság","pp","50","50","50","50"]
["","Modell","","","BYCQ140D7W1 - fehér szürke lamellákkal","BYCQ140D7W1 - fehér szürke lamellákkal","BYCQ140D7W1 - fehér szürke lamellákkal","BYCQ140D7W1 - fehér szürke lamellákkal"]
["","Szín","","","Hófehér (RAL 9010)","Hófehér (RAL 9010)","Hófehér (RAL 9010)","Hófehér (RAL 9010)"]
["","Tömeg","","kg","5.4","5.4","5.4","5.4"]
["Sound power level","Hűtés","","dB(A)","61","61","61"]
["","Fűtés","","dB(A)","61","61","61"]
["Méretek","Egység","Szélesség","pp","840","840","840","840"]
["","","Mélység","pp","840","840","840","840"]
["","","Magasság","pp","288","288","288","288"]
["Burkolat","Anyag","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["Tömeg","Egység","","kg","26.0","26.0","26.0","25.0"]
["Dekorációs panel","Súly","","kg","10","10","10"]
["","Modell","","","BYCQ140D7GFW1 - automatikus tisztító panel finom hálós szűrővel","BYCQ140D7GFW1 - automatikus tisztító panel finom hálós szűrővel","BYCQ140D7GFW1 - automatikus tisztító panel finom hálós szűrővel"]
["","Méretek","Magasság","pp","130","130","130"]
["","","Mélység","pp","950","950","950"]
["","","Szélesség","pp","950","950","950"]
["","Szín","","","Hófehér (RAL 9010)","Hófehér (RAL 9010)","Hófehér (RAL 9010)"]
["Power supply","fázis","","","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50/60","50/60","50/60","50/60"]
["","Megnevezés","","","VE","VE","VE","VE"]
["","Feszültség","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - A BYCQ140D7W1W készülék szigetelése fehér. Tájékoztatásul közöljük, hogy a fehér szigetelésen látszólag erősebb a piszok lerakódása, ezért nem tanácsos a BYCQ140D7W1W dekorációs elem beszerelése olyan környezetben, ahol fokozott szennyeződésnek van kitéve.","(1) - A BYCQ140D7W1W készülék szigetelése fehér. Tájékoztatásul közöljük, hogy a fehér szigetelésen látszólag erősebb a piszok lerakódása, ezért nem tanácsos a BYCQ140D7W1W dekorációs elem beszerelése olyan környezetben, ahol fokozott szennyeződésnek van kitéve.","(1) - A BYCQ140D7W1W készülék szigetelése fehér. Tájékoztatásul közöljük, hogy a fehér szigetelésen látszólag erősebb a piszok lerakódása, ezért nem tanácsos a BYCQ140D7W1W dekorációs elem beszerelése olyan környezetben, ahol fokozott szennyeződésnek van kitéve.","(1) - A BYCQ140D7W1W készülék szigetelése fehér. Tájékoztatásul közöljük, hogy a fehér szigetelésen látszólag erősebb a piszok lerakódása, ezért nem tanácsos a BYCQ140D7W1W dekorációs elem beszerelése olyan környezetben, ahol fokozott szennyeződésnek van kitéve."]
["","","","","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz","(2) - Fluor-tartalmú, az ózonréteget károsító gázt tartalmaz"]
["","","","","(3) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(3) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(3) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(3) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]
["Hangnyomás szint","Fűtés","Magas","dB(A)","","","","36"]
["","","Közepes","dB(A)","","","","33"]
["","","Alacsony","dB(A)","","","","29"]
["","Hűtés","Medium","dB(A)","","","","33"]
["","","Alacsony","dB(A)","","","","29"]
["","","Magas","dB(A)","","","","36"]
["Csőcsatlakozások","Gáz","Külső átm.","pp","","","","15.9"]
["","Ürítés","","","","","","VP25 (I.D. 25/O.D. 32)"]
["Sound power level","Hűtés","","dB(A)","","","","53"]
["","Fűtés","","dB(A)","","","","53"]
["Dekorációs panel","Súly","","kg","","","","10"]
["","Modell","","","","","","BYCQ140D7GFW1 - automatikus tisztító panel finom hálós szűrővel"]
["","Méretek","Magasság","pp","","","","130"]
["","","Mélység","pp","","","","950"]
["","","Szélesség","pp","","","","950"]
["","Szín","","","","","","Hófehér (RAL 9010)"]