{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H"]
[]
[]
[]
[]
["","","","","","FCAHG71HVEB","FCAHG100HVEB","FCAHG125HVEB","FCAHG140HVEB"]
["Hűtési teljesítmény","Hűtési összteljesítmény","","Névl.","kW","6.80","9.50","12.10","13.40"]
["Fűtési teljesítmény","Összes teljesítmény","","Névl.","kW","7.50","10.8","13.5","15.5"]
["Burkolat","Anyag","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["Méretek","Egység","","Magasság","mm","288","288","288","288"]
["","","","Szélesség","mm","840","840","840","840"]
["","","","Mélység","mm","840","840","840","840"]
["Tömeg","Egység","","","kg","25","25","25","25"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","23.6","32.2","34.4","34.4"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","18.8","25.7","27.3","27.3"]
["","","","Alacsony","m³/perc","13.7","19.1","21.2","21.2"]
["","","Fűtés","Magas","m³/perc","23.6","30.8","32.1","32.1"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","18.8","24.6","25.5","25.5"]
["","","Fűtés","Alacsony","m³/perc","13.7","18.3","19.7","19.7"]
["Hangteljesítményszint","Hűtés","","","dB(A)","53","61","61","61"]
["","Fűtés","","","dB(A)","53","61","61","61"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","36","44","45","45"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","39","40","41"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","29","33","35","37"]
["","Fűtés","","Magas","dB(A)","36","44","45","45"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","33","39","40","41"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","29","33","35","37"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","9.52","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","mm","15.9","15.9","15.9","15.9"]
["","Ürítés","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Dekorációs panel","Modell","","","","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B","BYCQ140E2W1, BYCQ140E2W1W, BYCQ140E2W1B"]
["","Méretek","","Magasság","mm","65","65","65","65"]
["","","","Szélesség","mm","950","950","950","950"]
["","","","Mélység","mm","950","950","950","950"]
["","Tömeg","","","kg","5.5","5.5","5.5","5.5"]
["Dekorációs panel 2","Modell","","","","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B","BYCQ140E2GFW1, BYCQ140E2GFW1B"]
["","Méretek","","Magasság","mm","148","148","148","148"]
["","","","Szélesség","mm","950","950","950","950"]
["","","","Mélység","mm","950","950","950","950"]
["","Tömeg","","","kg","10.3","10.3","10.3","10.3"]
["Dekorációs panel 3","Modell","","","","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB","BYCQ140E2P, BYCQ140E2PB"]
["","Méretek","","Magasság","mm","106","106","106","106"]
["","","","Szélesség","mm","950","950","950","950"]
["","","","Mélység","mm","950","950","950","950"]
["","Tömeg","","","kg","6.5","6.5","6.5","6.5"]
["Vezérlőrendszerek","Infrared remote control","","","","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB","BRC7FA532F, BRC7FB532F, BRC7FA532FB, BRC7FB532FB"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Operation manual","","","","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7"]
["","Clamp for drain hose","","","","1","1","1","1"]
["","Clamps","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation guide","","","","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2"]
["","Screws","","","","4","4","4","4"]
["","Sealing pads","","","","1","1","1","1"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Áramellátás-=-Frekvencia","","Frekvencia","","50/60","50/60","50/60","50/60"]
["","Áramellátás-=-Feszültség","","Feszültség","","220-240/220","220-240/220","220-240/220","220-240/220"]