{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG100FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / RZQG71L8Y1B","FCQG71FVEB / RZQG71L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG100L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG100L8Y1B","FCQG140FVEB / RZQG125L8Y1B","FCQG71FVEB / FCQG71FVEB / RZQG125L8Y1B","FCQG140FVEB / RZQG140L7Y1B"]
["Hűtési teljesítmény","Névl.","","kW","","","6.8","","","","","","","13.4"]
["Felülethűtés","SEER","","","6.80","5.1","6.72","5.10","5.10","5.10","6.80","6.00","5.10"]
["","Éves energiafogyasztás","","kWh/a","350","467","355","652","652","652","489","700","824"]
["","Kapacitás","Pdesign","kW","6.80","6.8","6.80","9.50","9.50","9.50","9.50","12.00","12.00"]
["","Energiatakarékossági osztály","","","A++","B","A++","B","B","B","A++","A+","B"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","6.33","6","6.33","11.30","11.30","11.30","11.30","12.66","12.71"]
["","SCOP/A","","","4.20","3.8","4.20","3.80","3.80","3.80","4.61","4.10","3.80"]
["","Energiatakarékossági osztály","","","A+","A","A+","A","A","A","A++","A+","A"]
["","Éves energiafogyasztás","","kWh/a","2,110","2,211","2,110","4,164","4,164","4,164","3,432","4,323","4,683"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","","1,005"]
["","EER","","","","","3.39","","","","","","","3.21"]
["","COP","","","","","3.97","","","","","","","3.61"]
["","Energiacímkézés irányelve","Hűtés","","","","A"]
["","","Fűtés","","","","A"]
["Fűtőkapacitás","Névl.","","kW","","","7.5","","","","","","","15.5"]
["Notes","","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","","","(1) - Az éves energiafogyasztás megfelel az 2002/31/EC energiafogyasztási direktívának","","","","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","","","(2) - A SEER és SCOP értékek megfelelnek az EN 14825 szabvány előírásainak","","","","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]