{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FDA125A5VEB / RZASG125M7V1B"]
["Hűtési teljesítmény","Névl.","","kW","12.1 (1)"]
["Fűtőkapacitás","Névl.","","kW","13.5 (2)"]
["Felülethűtés","Kapacitás","Pdesign","kW","12.1"]
["","SEER","","","5.03"]
["","Éves energiafogyasztás","","kWh/a","1,444"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","6.00"]
["","SCOP/A","","","3.58"]
["","Éves energiafogyasztás","","kWh/a","2,346"]
["Notes","","","","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","(4) - Az elektromos adatokat lásd külön rajzokon"]