{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Hűtési teljesítmény","Összes teljesítmény","","Névl.","kW","12.10","19.00","22.00"]
["Fűtőkapacitás","Összes teljesítmény","","Névl.","kW","13.50","22.4","24.0"]
["Burkolat","Colour","","","","Festetlen","Festetlen","Festetlen"]
["","Anyag","","","","Galvanizált acél","Galvanizált acéllemez","Galvanizált acéllemez"]
["Méretek","Egység","","Magasság","pp","300","470","470"]
["","","","Szélesség","pp","1,400","1,490","1,490"]
["","","","Mélység","pp","700","1,100","1,100"]
["Tömeg","Egység","","","kg","45","104","115"]
["Szükséges mennyezeti nyílás >","pp","","","","350"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","39.0","64.0","69.0"]
["","","","Medium","m³/perc","","50","56"]
["","","","Alacsony","m³/perc","28.0","36.0","43.0"]
["","","Fűtés","Magas","m³/perc","39.0","64.0","69.0"]
["","","","Medium","m³/perc","","50.0","56.0"]
["","","","Alacsony","m³/perc","28.0","36.0","43.0"]
["","Külső statikus nyomás","","Magas","Pa","200","250","250"]
["","","","Névl.","Pa","50","62","62"]
["Sound power level","Hűtés","","","dB(A)","66","69.0","71.0"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","40","43.0","44.0"]
["","","","Medium","dB(A)","","39.0","40.0"]
["","","","Alacsony","dB(A)","33","36.0","37.0"]
["","Fűtés","","Magas","dB(A)","40","43.0","44.0"]
["","","","Közepes","dB(A)","","39.0","40.0"]
["","","","Alacsony","dB(A)","33","36.0","37.0"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","9.52","9.52","9.52"]
["","Gáz","","Külső átm.","pp","15.90","19.1","22.2"]
["","Ürítés","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Leeresztési emelési magasság","pp","","","","625"]
["Dekorációs panel","Model","","","","BYBS125DJW1"]
["","Szín","","","","Fehér (10Y9/0,5)"]
["","Befoglaló méretek","","Magasság","pp","55"]
["","","","Szélesség","pp","1,500"]
["","","","Mélység","pp","500"]
["","Súly","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Használati utasítás","","","","","1","1"]
["","Telepítési és használati utasítás","","","","1","1","1"]
["","Telepítési utasítás","","","","","1","1"]
["","Általános biztonsági óvintézkedések","","","","1","1","1"]
["","Gázcsatlakozó cső","","","","","1","1"]
["","Vezetékbilincs anyag","","","","","1","1"]
["","Alátét","","","","8","12","12"]
["","Rugós alátét","","","","","2","2"]
["","Csavar+alátét","","","","","45","45"]
["","Hatlapfejű csavar alátéttel","","","","","49","49"]
["","Csavarok","","","","16","2","2"]
["","Hatlapfejű csavar","","","","","2","2"]
["","Lapos alátét","","","","","8","8"]
["Power supply","Megnevezés","","","","","VE","VE"]
["","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50/60","50/60","50/60"]
["","Feszültség","","","V","220-240/220","220-240/220","220-240/220"]
["Standard Accessories","Tömlősáv","","","","1"]
["","Leeresztő tömlő","","","","1"]
["","Vezeték a közös áramellátáshoz","","","","2"]
["","Tömítőanyag (leeresztő tömlő)","","","","1"]
["","Tömítő anyag","","","","2"]
["","Hőszigetelő cső (folyadék)","","","","1"]
["","Hőszigetelő cső (gáz)","","","","1"]
["Notes","","","","","(1) - Az elektromos adatokat lásd külön rajzokon"]