{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","35.0","35.0"]
["","","","Alacsony","dB(A)","29.0","29.0"]
["","Hűtés","","Alacsony","dB(A)","28.0","28.0"]
["","","","Magas","dB(A)","35.0","35.0"]
["Standard Accessories","Telepítési és használati utasítás","","","","1","1"]
["","Szívási légszűrő","","","","1","1"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC1D52, BRC1E52A/B"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35"]
["","Gáz","","Külső átm.","mm","9.52"]
["","Ürítés","","","","27.2"]
["Sound power level","Hűtés","","","dB(A)","55","55"]
["","Fűtés","","","dB(A)","55","55"]
["Méretek","Egység","","Szélesség","mm","652","652"]
["","","","Mélység","mm","502","502"]
["","","","Magasság","mm","230","230"]
["Burkolat","Anyag","","","","Cinkbevonatú alacsony széntartalmú acél","Cinkbevonatú alacsony széntartalmú acél"]
["Tömeg","Egység","","","kg","17.0","17.0"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","","6.95"]
["","","","Alacsony","m³/perc","","5.20"]
["","","Hűtés","Alacsony","m³/perc","","5.20"]
["","","","Magas","m³/perc","","6.50"]
["Power supply","fázis","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Megnevezés","","","","V1","V1"]
["","Feszültség","","","V","230","230 +/-10%"]
["Notes","","","","","(1) - A hangértékek mérése félig visszhangmentes helyiségben történik.","(1) - A hangértékek mérése félig visszhangmentes helyiségben történik."]
["","","","","","(2) - A hangnyomás szintje egy relatív érték, mely a hangforrás távolságától és az akusztikai környezettől függ. További részletekért, tekintse meg a hangerőszintek diagramjait.","(2) - A hangnyomás szintje egy relatív érték, mely a hangforrás távolságától és az akusztikai környezettől függ. További részletekért, tekintse meg a hangerőszintek diagramjait."]
["","","","","","(3) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(3) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","6.35"]
["","Gáz","","Külső átm.","mm","","9.52"]
["","Ürítés","","","","","27.2"]