{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-DV1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D7V1B"]
["Hűtési teljesítmény","Névl.","","kW","12.5 (1)"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","9.52"]
["","Gáz","Külső átm.","pp","15.9"]
["","Ürítés","OD","pp","26"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Energiacímkézés irányelve","Hűtés","","B"]
["","","Fűtés","","A"]
["Fűtőkapacitás","Névl.","","kW","14.0 (2)"]
["Notes","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 5 m; szintkülönbség: 0m"]
["","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5 m; szintkülönbség: 0m"]
["","","","","(3) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]