{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQSG125L9V1B (Archived)","FDQ125C7VEB / RZQSG125L9V1B (Archived)"]
["Hűtési teljesítmény","Névl.","","kW","12.0","12.0"]
["Fűtőkapacitás","Névl.","","kW","13.5","13.5"]
["Normál hatékonyság","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Annual energy consumption","","kWh","1,870","1,870"]
["","Energiacímkézés irányelve","Hűtés","","A","A"]
["","","Fűtés","","B","B"]
["Felülethűtés","Energiatakarékossági osztály","","","A","A"]
["","Kapacitás","Pdesign","kW","12.00","12.00"]
["","SEER","","","5.20","5.20"]
["","Éves energiafogyasztás","","kWh/a","808","808"]
["Felületfűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A","A"]
["","Kapacitás","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.90","3.90"]
["","Éves energiafogyasztás","","kWh/a","2,729","2,729"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]