{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":9,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F"]
[]
[]
[]
[]
["","","","","","FDXM25F2V1B","FDXM35F2V1B","FDXM50F2V1B","FDXM60F2V1B"]
["Ventilátor","Légáramlási arány","Hűtés","Névl.","m³/perc","8.0","8.0","11.0","14.8"]
["Hangnyomás szint","Hűtés","","Névl.","dB(A)","33","33","36","35"]
["Ventilátor","Légáramlási arány","Fűtés","Névl.","m³/perc","8.0","8.0","14.8","14.8"]
["Hangnyomás szint","Fűtés","","Névl.","dB(A)","33","33","36","36"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.036","0.036","0.060","0.060"]
["","Fűtés","","Névl.","kW","0.036","0.036","0.060","0.060"]
["Méretek","Egység","","Magasság","mm","200","200","200","200"]
["","","","Szélesség","mm","750","750","1150","1150"]
["","","","Mélység","mm","620","620","620","620"]
["Tömeg","Egység","","","kg","21","21","30","30"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","8.7","8.7","12.0","16.0"]
["","","","Alacsony","m³/perc","7.3","7.3","10.0","13.5"]
["","","Fűtés","Magas","m³/perc","8.7","8.7","16.0","16.0"]
["","","","Alacsony","m³/perc","7.3","7.3","13.5","13.5"]
["","Külső statikus nyomás","","Névl.","Pa","30","30","40","40"]
["Hangteljesítményszint","Hűtés","","","dB(A)","53","53","55","56"]
["","Fűtés","","","dB(A)","53","53","55","56"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","35","35","38","38"]
["","","","Alacsony","dB(A)","27","27","30","30"]
["","Fűtés","","Magas","dB(A)","35","35","38","38"]
["","","","Alacsony","dB(A)","27","27","30","30"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5","12.7","12.7"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["","Vezetékes távszabályzó","","","","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A","BRC1D52, BRC1E51A"]
["Áramellátás","Megnevezés","","","","V1","V1","V1","V1"]
["","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","230","230","220-240","220-240"]