{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-R9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXM25R5V1B9","FDXM35F3V1B9 / RXM35R5V1B9"]
["Hűtési teljesítmény","Min.","","kW","1.30","1.40"]
["","Névl.","","kW","2.40","3.40"]
["","Max.","","kW","3.00","3.80"]
["Fűtőkapacitás","Min.","","kW","1.30","1.40"]
["","Névl.","","kW","3.20","4.00"]
["","Max.","","kW","4.50","5.00"]
["Normál hatékonyság","EER","","","3.77","2.98"]
["","COP","","","4.00","3.48"]
["","Éves energiafogyasztás","","kWh","318","570"]
["","Energiacímkézés irányelve","Hűtés","","A","C"]
["","","Fűtés","","A","B"]
["Felülethűtés","Energiatakarékossági osztály","","","","A"]
["","Kapacitás","Pdesign","kW","","3.40"]
["","SEER","","","","5.26"]
["","Éves energiafogyasztás","","kWh/a","","226"]
["Felületfűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","A"]
["","Kapacitás","Pdesign","kW","","2.90"]
["","SCOP/A","","","","3.88"]
["","Éves energiafogyasztás","","kWh/a","","1,046"]
["Notes","","","","(1) - Az elektromos adatokat lásd külön rajzokon","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(2) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(4) - Az elektromos adatokat lásd külön rajzokon"]