{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","35.0","35.0","","38.0"]
["","","","Közepes","dB(A)","33.0","33.0","","35.0"]
["","","","Alacsony","dB(A)","27.0","27.0","","30.0"]
["","Hűtés","","Közepes","dB(A)","33.0","33.0","","35.0"]
["","","","Alacsony","dB(A)","27.0","27.0","","30.0"]
["","","","Magas","dB(A)","35.0","35.0","","38.0"]
["Standard Accessories","Telepítési utasítás","","","","1","1","","1"]
["","Használati utasítás","","","","1","1","","1"]
["","Szigetelés a szereléshez","","","","1","1","","1"]
["","Tömítőlemez","","","","1","1","","1"]
["","Bilincs fém","","","","1","1","","1"]
["","Leeresztő tömlő","","","","1","1","","1"]
["","Alátét a függesztőkerethez","","","","8","8","","8"]
["","Tömítő anyag","","","","2","2","","2"]
["","Bilincsek","","","","6","6","","6"]
["","Alátétrögzítő lemez","","","","4","4","","4"]
["","Csavarok a csőcsatlakozásokhoz","","","","1","1","","1"]
["","Légszűrő","","","","1","1","","1"]
["Piping connections","Folyadék","","Külső átm.","mm","6.35","6.35","","6.35"]
["","Gáz","","Külső átm.","mm","9.50","9.50","","12.70"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Áramfelvétel","Hűtés","","Névl.","kW","0.036","0.036","","0.060"]
["","Fűtés","","Névl.","kW","0.036","0.036","","0.060"]
["Hangteljesítmény szintje","Hűtés","","","dB(A)","53.0","53.0","","56.0"]
["","Fűtés","","","dB(A)","53.0","53.0","","56.0"]
["Méretek","Berendezés","","Szélesség","mm","750","750","","1,150"]
["","","","Mélység","mm","620","620","","620"]
["","","","Magasság","mm","200","200","","200"]
["Tömeg","Egység","","","kg","21","21","","28"]
["Ventilátor","Külső statikus nyomás","","Névl.","Pa","30","30","","40"]
["","Légáramlási arány","Fűtés","Magas","m³/perc","8.7","8.7","","16.0"]
["","","","Medium","m³/perc","8.0","8.0","","14.8"]
["","","","Alacsony","m³/perc","7.3","7.3","","13.5"]
["","","Hűtés","Alacsony","m³/perc","7.3","7.3","","13.5"]
["","","","Medium","m³/perc","8.0","8.0","","14.8"]
["","","","Magas","m³/perc","8.7","8.7","","16.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Frekvencia","","","Hz","50","50","","50"]
["","Feszültség","","","V","220-240","220-240","","220-240"]
["Notes","","","","","(1) - Az elektromos adatokat lásd külön rajzokon","(1) - Az elektromos adatokat lásd külön rajzokon","","(1) - Az elektromos adatokat lásd külön rajzokon"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","","0.060"]
["","Fűtés","","Névl.","kW","","","0.060"]
["Méretek","Egység","","Magasság","mm","","","200"]
["","","","Szélesség","mm","","","1150"]
["","","","Mélység","mm","","","620"]
["Tömeg","Egység","","","kg","","","28"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","","15.8"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","","14.6"]
["","","","Alacsony","m³/perc","","","13.3"]
["","","Fűtés","Magas","m³/perc","","","15.8"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","","14.6"]
["","","Fűtés","Alacsony","m³/perc","","","13.3"]
["","Külső statikus nyomás","","Névl.","Pa","","","40"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","","55.0"]
["","Fűtés","","","dB(A)","","","55.0"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","","38.0"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","","35.0"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","","30.0"]
["","Fűtés","","Magas","dB(A)","","","38.0"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","","35.0"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","","30.0"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","","","6.35"]
["","Gáz","","Külső átm.","mm","","","12.70"]
["","Ürítés","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Légszűrő","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Áramellátás","fázis","","","","","","1~"]
["","Frekvencia","","","Hz","","","50"]
["","Feszültség","","","V","","","220-240"]