{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Hűtési teljesítmény","Névl.","","kW","2.40 (3)"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","6.35"]
["","Gáz","Külső átm.","pp","9.5"]
["","Ürítés","OD","pp","VP20 (Külső átm.26, Belső átm. 20)"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","345"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Energiacímkézés irányelve","Hűtés","","A"]
["","","Fűtés","","B"]
["Fűtőkapacitás","Névl.","","kW","3.20 (4)"]
["Notes","","","","(1) - Energetikai címke: A-tól (leginkább energiatakarékos) G-ig (legkevésbé energiatakarékos)"]
["","","","","(2) - Éves energiafogyasztás: évi 500 órás, teljes terhelésen történő használatra alapul (névleges körülmények)"]
["","","","","(3) - Hűtés: belső hőm. 27°CDB, 19,0°CWB; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 5 m; szintkülönbség: 0m"]
["","","","","(4) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5 m; szintkülönbség: 0m"]
["","","","","(5) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]