{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60F2VEB / RXS60F4V1B"]
["Hűtési teljesítmény","Min.","","kW","1.7"]
["","Max.","","kW","6.5"]
["","Névl.","","kW","6.0 (2)"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35"]
["","Gáz","Külső átm.","mm","12.7"]
["","Drain","OD","mm","VP20 (Külső átm.26, Belső átm. 20)"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","1,030"]
["","EER","","","2.91 (1)"]
["","COP","","","3.21 (1)"]
["","Energiacímkézés irányelve","Hűtés","","C"]
["","","Fűtés","","C"]
["Fűtőkapacitás","Névl.","","kW","7.0 (3)"]
["","Min.","","kW","1.7"]
["","Max.","","kW","8.0"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - Hűtés: belső hőm. 27°CDB, 19,0°CWB; kültéri hőm. 35°C száraz hőm., 24°C nedves hőm.; egyenlő csőhossz: 5m"]
["","","","","(3) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 5m"]
["","","","","(4) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]