{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Hűtési teljesítmény","Névl.","","kW","","5.70"]
["Fűtőkapacitás","Névl.","","kW","","7.00"]
["Normál hatékonyság","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Éves energiafogyasztás","","kWh","","934"]
["","Energiacímkézés irányelve","Hűtés","","","B"]
["","","Fűtés","","","B"]
["Felülethűtés","Energiatakarékossági osztály","","","","A+"]
["","Kapacitás","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Éves energiafogyasztás","","kWh/a","","347"]
["Felületfűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","A+"]
["","Kapacitás","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Éves energiafogyasztás","","kWh/a","","1,372"]
["Notes","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Hűtési teljesítmény","Névl.","","kW","5.00"]
["Fűtőkapacitás","Névl.","","kW","5.80"]
["Névleges hatékonyság","EER","","","3.24"]
["","COP","","","3.49"]
["","Éves energiafogyasztás","","kWh","771"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A"]
["","","Fűtés","","B"]
["Felülethűtés","Energiatakarékossági osztály","","","A+"]
["","Kapacitás","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Éves energiafogyasztás","","kWh/a","292"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A"]
["","Kapacitás","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","3.51"]
["","Éves energiafogyasztás","","kWh/a","1377"]
["Energiatakarékossági besorolás","","","","A+++ ~ D"]