{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Hűtési teljesítmény","Névl.","","kW","5.00","5.70"]
["Felülethűtés","Éves energiafogyasztás","","kWh/a","","347"]
["","Kapacitás","Pdesign","kW","","5.70"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","","3.96"]
["","Éves energiafogyasztás","","kWh/a","","1,372"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","771","934"]
["","EER","","","3.24","3.05"]
["","COP","","","3.49","3.41"]
["","Energiacímkézés irányelve","Hűtés","","A","B"]
["","","Fűtés","","B","B"]
["Fűtőkapacitás","Névl.","","kW","5.80","7.00"]
["Notes","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(3) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(4) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Felülethűtés","Energiatakarékossági osztály","","","","A+"]
["","SEER","","","","5.76"]
["Felületfűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","A+"]
["","SCOP/A","","","","4.04"]