{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / RZASG71M2V1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7V1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7V1B"]
["Hűtési teljesítmény","Névl.","","kW","6.80 (1)"]
["Felülethűtés","SEER","","","6.12"]
["","Éves energiafogyasztás","","kWh/a","389"]
["","Kapacitás","Pdesign","kW","6.80"]
["","Energiatakarékossági osztály","","","A++"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","4.50"]
["","SCOP/A","","","3.84"]
["","Energiatakarékossági osztály","","","A"]
["","Éves energiafogyasztás","","kWh/a","1,641"]
["Fűtőkapacitás","Névl.","","kW","7.50 (2)"]
["Notes","","","","(1) - Hűtés: T2: beltéri hőm. 26,6°CDB, 19,4°CWB, kültéri hőm. 48°C száraz hőm. [Btu/óra/W]","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["Outdoor unit","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Hűtési teljesítmény","Névl.","","kW","","9.50","9.50"]
["Fűtőkapacitás","Névl.","","kW","","10.8","10.8"]
["Felülethűtés","Energiatakarékossági osztály","","","","A++","A"]
["","Kapacitás","Pdesign","kW","","9.50","9.50"]
["","SEER","","","","6.24","5.49"]
["","Éves energiafogyasztás","","kWh/a","","533","606"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","A","A"]
["","Kapacitás","Pdesign","kW","","6.00","6.00"]
["","SCOP/A","","","","3.82","3.90"]
["","Éves energiafogyasztás","","kWh/a","","2199","2154"]