{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Burkolat","Anyag","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["Méretek","Egység","","Magasság","pp","260","260","260","260"]
["","","","Szélesség","pp","575","575","575","575"]
["","","","Mélység","pp","575","575","575","575"]
["Tömeg","Egység","","","kg","16.0","16.0","17.5","17.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9.0","10.0","12.0","14.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8.0","8.5","10.0","12.5"]
["","","","Alacsony","m³/perc","6.5","6.5","7.5","9.5"]
["","","Fűtés","Magas","m³/perc","9.0","10.0","12.0","14.5"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.0","8.5","10.0","12.5"]
["","","Fűtés","Alacsony","m³/perc","6.5","6.5","7.5","9.5"]
["Hangteljesítményszint","Hűtés","","","dB(A)","48","51","56","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","31.0","34.0","39.0","43.0"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","28.5","30.5","34.0","40.0"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25.0","25.0","27.0","32.0"]
["","Fűtés","","Magas","dB(A)","31.0","34.0","39.0","43.0"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","28.5","30.5","34.0","40.0"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","25.0","25.0","27.0","32.0"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.52","9.52","12.70","12.70"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Dekorációs panel","Modell","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Szín","","","","Fehér (N9.5)","Fehér (N9.5)","Fehér (N9.5)","Fehér (N9.5)"]
["","Méretek","","Magasság","pp","46","46","46","46"]
["","","","Szélesség","pp","620","620","620","620"]
["","","","Mélység","pp","620","620","620","620"]
["","Tömeg","","","kg","2.8","2.8","2.8","2.8"]
["Dekorációs panel 2","Modell","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Szín","","","","Ezüst","Ezüst","Ezüst","Ezüst"]
["","Méretek","","Magasság","pp","46","46","46","46"]
["","","","Szélesség","pp","620","620","620","620"]
["","","","Mélység","pp","620","620","620","620"]
["","Tömeg","","","kg","2.8","2.8","2.8","2.8"]
["Dekorációs panel 3","Modell","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Szín","","","","Fehér (RAL9010)","Fehér (RAL9010)","Fehér (RAL9010)","Fehér (RAL9010)"]
["","Méretek","","Magasság","pp","55","55","55","55"]
["","","","Szélesség","pp","700","700","700","700"]
["","","","Mélység","pp","700","700","700","700"]
["","Tömeg","","","kg","2.7","2.7","2.7","2.7"]
["Dekorációs panel 4","Modell","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Szín","","","","Fehér (RAL9010)","Fehér (RAL9010)","Fehér (RAL9010)","Fehér (RAL9010)"]
["","Méretek","","Magasság","pp","55","55","55","55"]
["","","","Szélesség","pp","700","700","700","700"]
["","","","Mélység","pp","700","700","700","700"]
["","Tömeg","","","kg","2.7","2.7","2.7","2.7"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","BRC7EB530 (szabványos panel), BRC7F530W (fehér panel), BRC7F530S (szürke panel)","BRC7EB530 (szabványos panel), BRC7F530W (fehér panel), BRC7F530S (szürke panel)","BRC7EB530 (szabványos panel), BRC7F530W (fehér panel), BRC7F530S (szürke panel)","BRC7EB530 (szabványos panel), BRC7F530W (fehér panel), BRC7F530S (szürke panel)"]
["","Vezetékes távszabályzó","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Áramellátás","fázis","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240"]