{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["Energiatakarékossági besorolás","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Hűtési teljesítmény","Névl.","","kW","","","","","","","","6.80","6.80","6.80"]
["Felülethűtés","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","467","467","467"]
["","Kapacitás","Pdesign","kW","","","","","","","","6.80","6.80","6.80"]
["","Energiatakarékossági osztály","","","","","","","","","","A","A","A"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Energiatakarékossági osztály","","","","","","","","","","A","A","A"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","2,211","2,211","2,211"]
["Normál hatékonyság","EER","","","","","","","","","","3.38","3.38","3.38"]
["Notes","","","","","","","","","","","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőmérséklet: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(1) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","","","","","","(2) - Az elektromos adatokat lásd külön rajzokon","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m.","(2) - Az elektromos adatokat lásd külön rajzokon"]
["","","","","","","","","","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","","","","","","","(4) - Az elektromos adatokat lásd külön rajzokon"]