{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B","FHA50AVEB99 / RXM50A5V1B","FHA60AVEB98 / RXM60A5V1B"]
["Hűtési teljesítmény","Névl.","","kW","5.00","5.00","5.7"]
["Fűtőkapacitás","Névl.","","kW","6.00","6.00","7.2"]
["Névleges hatékonyság","EER","","","3.21","3.21","3.29"]
["","COP","","","3.35","3.35","3.32"]
["","Éves energiafogyasztás","","kWh","779","779","866"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A","A","A"]
["","","Fűtés","","C","C","C"]
["Felülethűtés","Energiatakarékossági osztály","","","A+","A+","A+"]
["","Kapacitás","Pdesign","kW","5.00","5.00","5.7"]
["","SEER","","","5.92","5.92","6.08"]
["","Éves energiafogyasztás","","kWh/a","295","295","328"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A","A","A"]
["","Kapacitás","Pdesign","kW","4.35","4.35","4.71"]
["","SCOP/A","","","3.86","3.86","3.87"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","3.85","3.85","4.08"]
["","Éves energiafogyasztás","","kWh/a","1577","1577","1704"]
["Notes","","","","","","(1) - A névleges hűtési teljesítmények a következő feltételekre vonatkoznak: belső hőmérséklet: 27 °C száraz hőm., 19 °C nedves hőm., kültéri hőm.: 35°C száraz, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","","(2) - A névleges fűtési kapacitás alapja: belső hőmérséklet: 20°C száraz, kültéri hőmérséklet: 7 °C száraz, 6 °C párás, a hűtőközeg egyenértékű csővezetékhossza: 5m, szintkülönbség: 0m."]
["","","","","","","(3) - Az üzemi tartomány tekintetében ld. az önálló ábrát"]
["","","","","","","(4) - Az elektromos adatokat lásd külön rajzokon"]