{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RZAG-B"]
[]
[]
[]
[]
["","","","","FHA35AVEB98 / RZAG35B5V1B","FHA50AVEB98 / RZAG35B5V1B","FHA50AVEB98 / RZAG50B5V1B","FHA60AVEB98 / RZAG50B5V1B","FHA60AVEB98 / RZAG60B5V1B","FHA71AVEB98 / RZAG60B5V1B"]
["Hűtési teljesítmény","Min.","","kW","1.7","1.7","1.7","1.7","1.9","1.9"]
["","Névl.","","kW","3.5","3.5","5","5","6","6"]
["","Max.","","kW","4.5","4.5","6","6","6.8","6.8"]
["Fűtőkapacitás","Min.","","kW","1.4","1.4","1.7","1.7","1.7","1.7"]
["","Névl.","","kW","4","4","5.8","6","7","7"]
["","Max.","","kW","5.5","5.5","6.5","6.5","7.5","7.5"]
["Névleges hatékonyság","EER","","","4.6","5.05","4.1","4.24","3.9","4.35"]
["","COP","","","4.1","4.18","3.71","3.75","3.4","3.52"]
["","Éves energiafogyasztás","","kWh","380","347","610","590","769","690"]
["Normál hatékonyság","Energiacímkézés irányelve","Hűtés","","A","A","A","A","A","A"]
["","","Fűtés","","A","A","A","A","C","B"]
["Felülethűtés","Energiatakarékossági osztály","","","A++","A++","A++","A++","A++","A++"]
["","Kapacitás","Pdesign","kW","3.5","3.5","5","5","6","6"]
["","SEER","","","6.4","6.65","6.8","7.02","6.6","6.81"]
["","Éves energiafogyasztás","","kWh/a","191","184","257","249","318","308"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","A+","A+","A+","A+","A+","A+"]
["","Kapacitás","Pdesign","kW","3.1","3.1","4","4","4.6","4.6"]
["","SCOP/A","","","4.1","4.18","4.3","4.44","4.2","4.35"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","2.75","2.77","3.46","3.48","3.93","3.96"]
["","Éves energiafogyasztás","","kWh/a","1058","1038","1302","1261","1633","1480"]