{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG125L8Y1B","FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA60AVEB / FHA60AVEB / RZQG125L8Y1B","FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA50AVEB / FHA50AVEB / RZQG71L8Y1B","FHA71AVEB / RZQG71L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG71L8Y1B","FHA71AVEB / FHA71AVEB / RZQG100L8Y1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZQG100L8Y1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZQG100L8Y1B","FHA71AVEB / FHA71AVEB / RZQG125L8Y1B"]
["Energiatakarékossági besorolás","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","","","","","A+++ ~ D"]
["Felülethűtés","SEER","","","","","","","","5.10","5.10","6.86","5.10","5.10","5.10","5.10"]
["","Éves energiafogyasztás","","kWh/a","","","","","","467","467","347","467","652","652","652"]
["","Kapacitás","Pdesign","kW","","","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50"]
["","Energiatakarékossági osztály","","","","","","","","A","A","A++","A","A","A","A"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","","","","","","6.00","6.00","7.60","6.00","11.30","11.30","11.30"]
["","SCOP/A","","","","","","","","3.80","3.80","4.32","3.80","3.80","3.80","3.80"]
["","Energiatakarékossági osztály","","","","","","","","A","A","A+","A","A","A","A"]
["","Éves energiafogyasztás","","kWh/a","","","","","","2,211","2,211","2,463","2,211","4,164","4,164","4,164"]
["Notes","","","","","","","","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m","","(1) - Hűtés: belső hőm. 27 °C száraz, 19 °C nedves hőm.; kültéri hőm. 35°C száraz hőmérséklet; egyenlő csőhossz: 7,5m; szintkülönbség: 0m"]
["","","","","","","","","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m","","(2) - Fűtés: belső hőm. 20°C száraz hőm.; külső hőm. 7 °C száraz hőm., 6 °C nedves hőm.; a hűtőközeg egyenértékű csővezetékhossza: 7,5m; szintkülönbség: 0m"]
["","","","","","","","","","(3) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","(3) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["Hűtési teljesítmény","Névl.","","kW","","","","","","","","6.80 (1)"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","","","","","","","890"]
["","EER","","","","","","","","","","3.82 (3)"]
["","COP","","","","","","","","","","4.13 (3)"]
["","Energiacímkézés irányelve","Hűtés","","","","","","","","","A"]
["","","Fűtés","","","","","","","","","A"]
["Fűtőkapacitás","Névl.","","kW","","","","","","","","7.50 (2)"]
["Felülethűtés","Energiatakarékossági osztály","","","","","","","","","","","","","","","A"]
["","Kapacitás","Pdesign","kW","","","","","","","","","","","","","12.00"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","","","","","824"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","","","","","","","","","","","","A"]
["","Kapacitás","Pdesign","kW","","","","","","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Pdh fűtőteljesítmény -10 ° hőmérsékleten","","kW","","","","","","","","","","","","","11"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","","","","","","4683"]