{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","36","37","37","38"]
["","","Névl.","dB(A)","34","35","35","36"]
["","","Közepes","dB(A)","31","32","33","34"]
["","Hűtés","Közepes","dB(A)","34","35","35","36"]
["","","Alacsony","dB(A)","31","32","33","34"]
["","","Magas","dB(A)","36","37","37","38"]
["Standard Accessories","Hőszigetelő cső","","","2","2","2","2"]
["","Vezetékbilincs anyag","","","7","7","7","7"]
["","Tömlősáv","","","1","1","1","1"]
["","Leeresztő tömlő","","","1","1","1","1"]
["","Alátét","","","8","8","8","8"]
["","Tömítőlemez (nagyméretű)","","","1","1","1","1"]
["","Tömítőlemez (kisméretű)","","","1","1","1","1"]
["","Műgyanta persely","","","1","1","1","1"]
["","Csavarok","","","2","2","2","2"]
["","Vezetékrögzítő","","","2","2","2","2"]
["Vezérlőrendszerek","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35","6.35","6.35","9.52"]
["","Gáz","Külső átm.","mm","9.50","12.7","12.7","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20"]
["Hangteljesítményszint","Hűtés","","dB(A)","53","54","54","55"]
["Méretek","Egység","Szélesség","mm","960","960","1,270","1,270"]
["","","Mélység","mm","690","690","690","690"]
["","","Magasság","mm","235","235","235","235"]
["Burkolat","Anyag","","","Műgyanta, fémlemez","Műgyanta, fémlemez","Műgyanta, fémlemez","Műgyanta, fémlemez"]
["","Szín","","","Fehér","Fehér","Fehér","Fehér"]
["Tömeg","Egység","","kg","24.0","25.0","31.0","32.0"]
["Power supply","fázis","","","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50","50","50","50"]
["","Feszültség","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Az elektromos adatokat lásd külön rajzokon","(1) - Az elektromos adatokat lásd külön rajzokon","(1) - Az elektromos adatokat lásd külön rajzokon","(1) - Az elektromos adatokat lásd külön rajzokon"]