{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FHQ100CAVEB / RZQG71L9V1B","FHQ71CAVEB / RZQG71L9V1B","FHQ100CAVEB / RZQG100L9V1B","FHQ140CAVEB / RZQG100L9V1B","FHQ125CAVEB / RZQG125L9V1B","FHQ140CAVEB / RZQG125L9V1B","FHQ140CAVEB / RZQG140L9V1B","FHQ71CAVEB / FHQ71CAVEB / RZQG125L9V1B (Archived)"]
["Hűtési teljesítmény","Névl.","","kW","","6.8","9.5","","12.0","","13.4"]
["Felülethűtés","SEER","","","6.95","6.95","6.11","6.11","6.01","6.01"]
["","Éves energiafogyasztás","","kWh/a","343","343","545","545","699","699"]
["","Kapacitás","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Energiatakarékossági osztály","","","A++","A++","A++","A++","A+","A+"]
["Felületfűtés (Mérsékelt éghajlat)","Kapacitás","Pdesign","kW","7.60","7.60","11.30","11.30","14.13","14.13"]
["","SCOP/A","","","4.32","4.32","4.61","4.61","4.23","4.23"]
["","Energiatakarékossági osztály","","","A+","A+","A++","A++","A+","A+"]
["","Éves energiafogyasztás","","kWh/a","2,463","2,463","3,432","3,432","4,677","4,677"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","","890","1,245","","1,790"]
["","EER","","","","3.82","3.81","","3.35","","3.31"]
["","COP","","","","4.13","4.15","","3.89","","3.63"]
["","Energiacímkézés irányelve","Hűtés","","","A","A","","A"]
["","","Fűtés","","","A","A","","A"]
["Fűtőkapacitás","Névl.","","kW","","7.5","10.8","","13.5","","15.5"]
["Notes","","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]
["Outdoor unit","","","","","","","","","","","RZQG125L9V1"]
["Felülethűtés","Energiatakarékossági osztály","","","","","","","","","","B"]
["","Kapacitás","Pdesign","kW","","","","","","","","12.00"]
["","SEER","","","","","","","","","","5.10"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","824"]
["Felülethűtés (Mérsékelt éghajlat)","Energiatakarékossági osztály","","","","","","","","","","A"]
["","Kapacitás","Pdesign","kW","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","3.80"]
["","Éves energiafogyasztás","","kWh/a","","","","","","","","4683"]