{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RXS-L3"]
[]
[]
[]
[]
["","","","","FHQ35CBVEB / RXS35L3V1B"]
["Hűtési teljesítmény","Névl.","","kW","3.4"]
["Normál hatékonyság","Éves energiafogyasztás","","kWh","459"]
["","EER","","","3.70 (1)"]
["","COP","","","4.08 (1)"]
["","Energiacímkézés irányelve","Hűtés","","A"]
["","","Fűtés","","A"]
["Fűtőkapacitás","Névl.","","kW","4.00 (2)"]
["Notes","","","","(1) - EER/COP értékek az Eurovent 2012 szerint, csak EU-n kívüli országokra vonatkozóan"]
["","","","","(2) - Névleges hatékonyság: hűtés 35°/27° névleges terhelésen, fűtés 7°/20° névleges terhelésen"]