{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","46"]
["","","Csendes működés","dB(A)","30"]
["","","Alacsony","dB(A)","33"]
["","Hűtés","Csendes működés","dB(A)","29"]
["","","Alacsony","dB(A)","32"]
["","","Magas","dB(A)","38"]
["","","Névl.","dB(A)","36"]
["","Hűtés","Névl.","dB(A)","35"]
["Standard Accessories","Telepítési utasítás","","","1"]
["","Használati utasítás","","","1"]
["","Infravörös távirányító","","","1"]
["","AAA szárazelemek","","","2"]
["","Távirányító tartó","","","1"]
["","Szerelőlemez","","","1"]
["","Hőszigetelő cső (hűtőcső)","","","8"]
["","Légtisztító szűrő","","","1"]
["","Fotokatalitikus szagtalanító szűrő","","","1"]
["","Oldalsó burkolat","","","2"]
["","Armatúraabroncs","","","4"]
["Control systems","Infrared remote control","","","ARC433B67"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","6.35"]
["","Gáz","Külső átm.","pp","9.5"]
["","Ürítés","","","18"]
["Sound power level","Hűtés","","dB(A)","53"]
["","Fűtés","","dB(A)","59"]
["Méretek","Egység","Szélesség","pp","1,050"]
["","","Mélység","pp","200"]
["","","Magasság","pp","490"]
["Burkolat","Colour","","","Mandula fehér"]
["Tömeg","Egység","","kg","16"]
["Power supply","fázis","","","1~"]
["","Frekvencia","","Hz","50"]
["","Megnevezés","","","VM"]
["","Feszültség","","V","220-240"]
["Notes","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]
["","","","","(4) - Multi rendszerű kültéri egységhez való csatlakoztatás esetén lásd a csatlakoztatandó multi kültéri egység műszaki jellemzőit"]