{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","33.0","33.0","36.0","36.0"]
["","","","Névl.","dB(A)","31.0","31.0","33.0","33.0"]
["","","","Alacsony","dB(A)","28.0","28.0","30.0","30.0"]
["","Hűtés","","Közepes","dB(A)","31.0","31.0","33.0","33.0"]
["","","","Alacsony","dB(A)","28.0","28.0","30.0","30.0"]
["","","","Magas","dB(A)","33.0","33.0","36.0","36.0"]
["Vezérlőrendszerek","Vezetékes távszabályzó","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.52","9.52","12.7","12.7"]
["","Ürítés","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Hűtés","","","dB(A)","53.0","53.0","56.0","56.0"]
["Méretek","Egység","","Szélesség","mm","790","790","1,190","1,190"]
["","","","Mélység","mm","200","200","200","200"]
["","","","Magasság","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Burkolat","Anyag","","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["","Szín","","","","Festetlen","Festetlen","Festetlen","Festetlen"]
["Tömeg","Egység","","","kg","23.0","23.0","30.0","30.0"]
["Ventilátor","Külső statikus nyomás","","Magas","Pa","48","48","49","49"]
["","","","Névl.","Pa","30","30","40","40"]
["","Légáramlási arány","Fűtés","Magas","m³/perc","8.7","8.7","16.0","16.0"]
["","","","Alacsony","m³/perc","7.3","7.3","13.5","13.5"]
["","","","Névl.","m³/perc","8.0","8.0","14.8","14.8"]
["","","Hűtés","Alacsony","m³/perc","7.3","7.3","13.5","13.5"]
["","","","Névl.","m³/perc","8.0","8.0","14.8","14.8"]
["","","","Magas","m³/perc","8.7","8.7","16.0","16.0"]
["Power supply","fázis","","","","1~","1~","1~","1~"]
["","Megnevezés","","","","VE","VE","VE","VE"]
["","Frekvencia","","","Hz","50/60","50/60","50/60","50/60"]
["","Feszültség","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - Tartólábakkal","(1) - Tartólábakkal","(1) - Tartólábakkal","(1) - Tartólábakkal"]
["","","","","","(2) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(2) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(2) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(2) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]