{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","33","33","36","36"]
["","","Névl.","dB(A)","31","31","33","33"]
["","","Alacsony","dB(A)","28","28","30","30"]
["","Hűtés","Alacsony","dB(A)","28","28","30","30"]
["","","Magas","dB(A)","33","33","36","36"]
["","","Névl.","dB(A)","31","31","33","33"]
["Hűtőközeg","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Vezérlőrendszerek","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Hűtési teljesítmény","Összes teljesítmény","Névl.","kW","2.6","3.4","5.0","6.0"]
["Piping connections","Folyadék","Külső átm.","mm","6.35","6.35","6.35","6.35"]
["","Gáz","Külső átm.","mm","9.52","9.52","12.7","12.7"]
["","Ürítés","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Hangteljesítmény szintje","Hűtés","","dB(A)","53","53","56","56"]
["Méretek","Berendezés","Szélesség","mm","790","790","1,190","1,190"]
["","","Mélység","mm","200","200","200","200"]
["","","Magasság","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Burkolat","Anyag","","","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez","Galvanizált acéllemez"]
["","Colour","","","Festetlen","Festetlen","Festetlen","Festetlen"]
["Tömeg","Egység","","kg","23","23","30","30"]
["Ventilátor","Külső statikus nyomás","Magas","Pa","48","48","49","49"]
["","","Névl.","Pa","30","30","40","40"]
["Fűtőkapacitás","Összes teljesítmény","Névl.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50/60","50/60","50/60","50/60"]
["","Feszültség","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték.","(1) - A hangteljesítmény szintje a hangforrás által generált teljesítményt jelző abszolút érték."]
["","","","","(2) - Tartólábakkal","(2) - Tartólábakkal","(2) - Tartólábakkal","(2) - Tartólábakkal"]