{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","42","44","46","39","40","41"]
["","","Csendes működés","dB(A)","30","32","34","25","25","26"]
["","","Alacsony","dB(A)","33","35","37","28","28","29"]
["","Hűtés","Csendes működés","dB(A)","31","33","34","22","22","23"]
["","","Alacsony","dB(A)","34","36","37","25","26","27"]
["","","Magas","dB(A)","43","45","46","39","40","41"]
["","","Névl.","dB(A)","38","40","42","34","34","35"]
["","Hűtés","Névl.","dB(A)","39","41","42","33","33","34"]
["Standard Accessories","Telepítési utasítás","","","1","1","1","1","1","1"]
["","Használati utasítás","","","1","1","1","1","1","1"]
["","Vezeték nélküli távirányító","","","1","1","1","1","1","1"]
["","Elemek","","","2","2","2","2","2","2"]
["","Távirányító tartó","","","1","1","1","1","1","1"]
["","Szerelőlemez","","","1","1","1","1","1","1"]
["","A beltéri egység rögzítő csavarja","","","","","","2","2","2"]
["","Titánium apatit fotokatalitikus légtisztító szűrő","","","2","2","2","2","2","2"]
["Vezérlőrendszerek","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Csőcsatlakozások","Folyadék","Külső átm.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gáz","Külső átm.","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Ürítés","","","18","18","18","18","18","18"]
["Elektromos bemenet","Hűtés","Névl.","kW","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Fűtés","Névl.","kW","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Hangteljesítményszint","Hűtés","","dB(A)","59","60","63","55","56","57"]
["","Fűtés","","dB(A)","58","59","62","55","56","57"]
["Méretek","Egység","Szélesség","mm","1,050","1,050","1,050","770","770","770"]
["","","Mélység","mm","238","238","238","198","198","198"]
["","","Magasság","mm","290","290","290","283","283","283"]
["Burkolat","Szín","","","Fehér","Fehér","Fehér","Fehér","Fehér","Fehér"]
["Tömeg","Egység","","kg","12","12","12","7","7","7"]
["Power supply","fázis","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","Hz","50","50","50","50","50","50"]
["","Megnevezés","","","V1","V1","V1","V1","V1","V1"]
["","Feszültség","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Beltéri egység rögzítő csavarja","","","2","2"]
["Notes","","","","(1) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje","(1) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje","(1) - SL: A Légszállítási sebesség beállításának néma ventilátorszintje"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["Standard Accessories","Beltéri egység rögzítő csavarjai (M4x12L)","","","","","2"]