{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":8,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3"]
[]
[]
[]
[]
["","","","","","FTX20J3V1B","FTX25J3V1B","FTX35J3V1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.03","0.030","0.030"]
["","Fűtés","","Névl.","kW","0.04","0.040","0.040"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér"]
["Méretek","Egység","","Magasság","pp","198","198","198"]
["","","","Szélesség","pp","770","770","770"]
["","","","Mélység","pp","283","283","283"]
["Tömeg","Egység","","","kg","7","7.00","7.00"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","9.1","9.2","9.3"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","7.4","7.6","7.7"]
["","","","Alacsony","m³/perc","5.9","6.0","6.1"]
["","","","Csendes működés","m³/perc","4.7","4.8","4.9"]
["","","Fűtés","Magas","m³/perc","9.4","9.7","10.1"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","7.8","8.0","8.4"]
["","","Fűtés","Alacsony","m³/perc","6.3","6.3","6.7"]
["","","","Csendes működés","m³/perc","5.5","5.5","5.7"]
["Hangteljesítményszint","Hűtés","","","dB(A)","55","55","58"]
["","Fűtés","","","dB(A)","55","55","58"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39","40","41"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","33","34"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","26","27"]
["","","","Csendes működés","dB(A)","22","22","23"]
["","Fűtés","","Magas","dB(A)","39","40","41"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","34","34","35"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","28","28","29"]
["","","","Csendes működés","dB(A)","25","25","26"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","pp","9.5","9.50","9.50"]
["","Ürítés","","","","18","18","18"]
["Control systems","Infrared remote control","","","","ARC433A87","ARC433A87","ARC433A87"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Áramellátás","Megnevezés","","","","V1","V1","V1"]
["","fázis","","","","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240"]