{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Hangnyomás szint","Fűtés","","Magas","dB(A)","39","40","41","","46"]
["","","","Közepes","dB(A)","32","33","33","","42"]
["","","","Csendes működés","dB(A)","19","19","19","","24"]
["","","","Alacsony","dB(A)","25","25","25","","33"]
["","Hűtés","","Medium","dB(A)","32","33","33","","39"]
["","","","Csendes működés","dB(A)","19","19","19","","24"]
["","","","Alacsony","dB(A)","25","25","25","","31"]
["","","","Magas","dB(A)","39","40","41","","46"]
["Standard Accessories","Telepítési utasítás","","","","1","1","1","","1"]
["","Használati utasítás","","","","1","1","1","","1"]
["","Légszűrő","","","","2","2","2","","2"]
["","Infravörös távirányító","","","","1","1","1","","1"]
["","A távirányító rögzítésére szolgáló lap","","","","1","1","1","","1"]
["","Csavarzsák","","","","1","1","1","","1"]
["","Csavarfedél","","","","1","1","1","","1"]
["","AAA szárazelemek","","","","2","2","2","","2"]
["","Általános biztonsági óvintézkedések","","","","1","1","1","","1"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","","675.0"]
["Control systems","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","6.35","6.35","6.35","","6.35"]
["","Gáz","","Külső átm.","pp","9.50","9.50","9.50","","12.70"]
["","Ürítés","","","","18","18","18","","18"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.020","0.022","0.023","","0.030"]
["","Fűtés","","Névl.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Hűtés","","","dB(A)","57","57","60","","60"]
["Méretek","Egység","","Szélesség","pp","798","798","798","","798"]
["","","","Mélység","pp","189","189","189","","189"]
["","","","Magasság","pp","295","295","295","","295"]
["Burkolat","Colour","","","","Fehér","Fehér","Fehér","","Fehér"]
["Tömeg","Egység","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilátor","Légáramlási arány","Fűtés","Magas","m³/perc","10.9","11.1","11.5","","15.1"]
["","","","Medium","m³/perc","8.7","9.0","9.0","","11.1"]
["","","","Alacsony","m³/perc","6.4","6.4","6.4","","8.2"]
["","","","Csendes működés","m³/perc","4.5","4.5","4.5","","5.7"]
["","","Hűtés","Alacsony","m³/perc","6.1","6.1","6.1","","7.6"]
["","","","Medium","m³/perc","8.2","8.6","8.6","","10.4"]
["","","","Magas","m³/perc","11.0","11.5","11.9","","13.5"]
["","","","Csendes működés","m³/perc","4.6","4.6","4.6","","5.2"]
["Power supply","fázis","","","","1~","1~","1~","","1~"]
["","Megnevezés","","","","V1","V1","V1","","V1"]
["","Frekvencia","","","Hz","50","50","50","","50"]
["","Feszültség","","","V","220-240","220-240","220-240","","220-240"]
["Elektromos bemenet","Hűtés","","Névl.","kW","","","","0.028"]
["","Fűtés","","Névl.","kW","","","","0.036"]
["Burkolat","Szín","","","","","","","Fehér"]
["Méretek","Egység","","Magasság","pp","","","","295"]
["","","","Szélesség","pp","","","","798"]
["","","","Mélység","pp","","","","189"]
["Tömeg","Egység","","","kg","","","","11.50"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","","","","13.1"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","","","","9.8"]
["","","","Alacsony","m³/perc","","","","7.2"]
["","","","Csendes működés","m³/perc","","","","4.6"]
["","","Fűtés","Magas","m³/perc","","","","14.6"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","","","","10.5"]
["","","Fűtés","Alacsony","m³/perc","","","","7.7"]
["","","","Csendes működés","m³/perc","","","","5.2"]
["Hangteljesítményszint","Hűtés","","","dB(A)","","","","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","","","","45"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","","","","37"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","","","","29"]
["","","","Csendes működés","dB(A)","","","","21"]
["","Fűtés","","Magas","dB(A)","","","","45"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","","","","37"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","","","","29"]
["","","","Csendes működés","dB(A)","","","","21"]
["Hűtőközeg","GWP","","","","","","","675.0"]
["Csőcsatlakozások","Folyadék","","Külső átm.","pp","","","","6.35"]
["","Gáz","","Külső átm.","pp","","","","12.70"]
["","Ürítés","","","","","","","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","","","","ARC466A58"]
["","Vezetékes távszabályzó","","","","","","","BRC073"]
["Standard Accessories","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Légszűrő","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Áramellátás","Megnevezés","","","","","","","V1"]
["","fázis","","","","","","","1~"]
["","Frekvencia","","","Hz","","","","50"]
["","Feszültség","","","V","","","","220-240"]