{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CB"]
[]
[]
[]
[]
["","","","","","FTXA20C2V1BB","FTXA25C2V1BB","FTXA35C2V1BB","FTXA42C2V1BB","FTXA50C2V1BB"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.02","0.022","0.023","0.028","0.030"]
["","Fűtés","","Névl.","kW","0.02","0.02","0.22","0.036","0.039"]
["Burkolat","Szín","","","","Fekete","Fekete","Fekete","Fekete","Fekete"]
["Méretek","Egység","","Magasság","mm","295","295","295","295","295"]
["","","","Szélesség","mm","798","798","798","798","798"]
["","","","Mélység","mm","189","189","189","189","189"]
["Tömeg","Egység","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","11","11.5","11.9","13.1","13.5"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8.2","8.6","8.6","9.8","10.4"]
["","","","Alacsony","m³/perc","6.1","6.1","6.1","7.2","7.6"]
["","","","Csendes működés","m³/perc","4.6","4.6","4.6","4.6","5.2"]
["","","Fűtés","Magas","m³/perc","10.9","11.1","11.5","14.6","15.1"]
["","Légszállítási sebesség","Fűtés","Közepes","m³/perc","8.7","9","9","10.5","11.1"]
["","","Fűtés","Alacsony","m³/perc","6.4","6.4","6.4","7.7","8.2"]
["","","","Csendes működés","m³/perc","4.5","4.5","4.5","5.2","5.7"]
["Hangteljesítményszint","Hűtés","","","dB(A)","57","57","60","60","60"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","39","40","41","45","46"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","32","33","33","37","39"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","25","25","25","29","31"]
["","","","Csendes működés","dB(A)","19","19","19","21","24"]
["","Fűtés","","Magas","dB(A)","39","40","41","45","46"]
["Hangnyomásszint","Fűtés","","Közepes","dB(A)","32","33","33","37","42"]
["Hangnyomás szint","Fűtés","","Alacsony","dB(A)","25","25","25","29","33"]
["","","","Csendes működés","dB(A)","19","19","19","21","24"]
["Hűtőközeg","GWP","","","","675","675","675","675","675.0"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.5","9.5","9.5","9.5","12.70"]
["","Ürítés","","","","18","18","18","18","18"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC466A85","ARC466A85","ARC466A85","ARC466A85","ARC466A85"]
["","Vezetékes távszabályzó","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Légszűrő","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Áramellátás","Megnevezés","","","","V1","V1","V1","V1","V1"]
["","fázis","","","","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240"]