{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-E"]
[]
[]
[]
[]
["","","","","","FTXC20EV1B","FTXC25EV1B","FTXC35EV1B","FTXC50EV1B","FTXC60EV1B","FTXC71EV1B"]
["Elektromos bemenet","Hűtés","","Névl.","kW","0.595","0.765","1.045","1.55","1.89","2.38"]
["","Fűtés","","Névl.","kW","0.67","0.75","1.07","1.515","1.68","2.46"]
["Burkolat","Szín","","","","Fehér","Fehér","Fehér","Fehér","Fehér","Fehér"]
["","Anyag","","","","Nagy ütésállóságú polisztirol","Nagy ütésállóságú polisztirol","Nagy ütésállóságú polisztirol","Nagy ütésállóságú polisztirol","Nagy ütésállóságú polisztirol","Nagy ütésállóságú polisztirol"]
["Méretek","Egység","","Magasság","mm","288","288","288","288","297","297"]
["","","","Szélesség","mm","770","770","770","770","990","990"]
["","","","Mélység","mm","234","234","234","234","273","273"]
["Tömeg","Egység","","","kg","9.0","9.0","9.5","9.5","13.0","13.0"]
["Ventilátor","Légáramlási arány","Hűtés","Magas","m³/perc","10.8","10.8","11.1","12.5","20.4","20.4"]
["","Légszállítási sebesség","Hűtés","Közepes","m³/perc","8.1","8.1","8.7","9.9","14.5","14.5"]
["","","","Alacsony","m³/perc","6.1","6.1","6.4","8.1","12.5","12.5"]
["","","","Csendes működés","m³/perc","5.4","5.4","5.4","7.4","10.2","10.2"]
["Hangteljesítményszint","Hűtés","","","dB(A)","57","57","58","60","63","63"]
["Hangnyomás szint","Hűtés","","Magas","dB(A)","40","40","41","47","48","48"]
["Hangnyomásszint","Hűtés","","Közepes","dB(A)","33","33","34","39","42","42"]
["Hangnyomás szint","Hűtés","","Alacsony","dB(A)","26","26","26","33","38","38"]
["","","","Csendes működés","dB(A)","21","21","22","30","31","31"]
["Csőcsatlakozások","Folyadék","","Külső átm.","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gáz","","Külső átm.","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Ürítés","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Vezérlőrendszerek","Infravörös távszabályzó","","","","ARC486A6","ARC486A6","ARC486A6","ARC486A6","ARC486A6","ARC486A6"]
["Áramellátás","Megnevezés","","","","V1","V1","V1","V1","V1","V1"]
["","fázis","","","","1~","1~","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Feszültség","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]