{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Hangnyomás szint","Fűtés","Magas","dB(A)","39","40"]
["","","Közepes","dB(A)","34","34"]
["","","Csendes működés","dB(A)","21","21"]
["","","Alacsony","dB(A)","28","28"]
["","Hűtés","Közepes","dB(A)","33","33"]
["","","Csendes működés","dB(A)","20","20"]
["","","Alacsony","dB(A)","25","26"]
["","","Magas","dB(A)","39","40"]
["Standard Accessories","Telepítési utasítás","","","1","1"]
["","Használati utasítás","","","1","1"]
["","Infravörös távirányító","","","1","1"]
["","AAA szárazelemek","","","2","2"]
["","Távirányító tartó","","","1","1"]
["","Szerelőlemez","","","1","1"]
["","Beltéri egység rögzítő csavarja","","","2","2"]
["Control systems","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Csőcsatlakozások","Folyadék","Külső átm.","pp","6.35","6.35"]
["","Gáz","Külső átm.","pp","9.50","9.50"]
["","Ürítés","","","18","18"]
["Elektromos bemenet","Hűtés","Névl.","kW","0.017","0.019"]
["","Fűtés","Névl.","kW","0.020","0.020"]
["Hangteljesítmény szintje","Hűtés","","dB(A)","55","55"]
["","Fűtés","","dB(A)","55","55"]
["Méretek","Egység","Szélesség","pp","770","770"]
["","","Mélység","pp","225","225"]
["","","Magasság","pp","286","286"]
["Casing","Colour","","","Fehér","Fehér"]
["Tömeg","Egység","","kg","8.50","8.50"]
["Áramellátás","Phase","","","1~","1~"]
["","Frekvencia","","Hz","50","50"]
["","Feszültség","","V","220-240","220-240"]